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	TF-02
Initial Statement of Compliance Report - 
Control Combination or Idling Emission Limit Standards
Halogenated Solvent Cleaning Equipment
Air Quality Permit Program
Doc Type: Notification


Instructions: This report must be postmarked or received by the applicable due date, located at the bottom of this page. Submit completed report to both:
	Minnesota Pollution Control Agency
AQ Compliance Tracking Coordinator:
AQRoutineReport.PCA@state.mn.us

	George Czerniak
AE-17J
U.S. EPA Region 5
77 West Jackson Boulevard
Chicago, IL 60604-3507



	AI ID:
	[bookmark: Text118]     
	Date (mm/dd/yyyy):
	[bookmark: Text262]     

	Facility name:
	     


Facility address
	Street address:
	     
	County:
	[bookmark: Text2]     

	City:
	     
	State:
	     
	Zip code:
	     


Mailing address
	Street address:
	     
	
	

	City:
	     
	State:
	     
	Zip code:
	     



	Facility contact person:
	     
	Phone number:
	[bookmark: Text274]     

	Title:
	[bookmark: Text263]     
	


Responsible official
	Name:
	[bookmark: Text119]     
	
	

	Title:
	     
	
	

	Signature:
	
	Date (mm/dd/yyyy):
	[bookmark: Text264]     


Cleaning machine (fill out separate form for each solvent tank)
	1.
	Tank Identification No.:
	[bookmark: Text265]     
	

	
	Date of tank installation (mm/dd/yyyy):
	[bookmark: Text266]     
	

	
	Tank is:
	|_| Existing
	(This report is due by May 1, 1998)

	
	
	|_| New
	(This report is due 150 days after start-up or May 1, 1995, whichever is later)



	2.
	Type of machine:
	|_| Batch vapor
	

	
	
	|_| In-Line
	



	
	Solvent/Air Interface area:
	[bookmark: Text267]     
	square meters

	
	
	or
	

	
	
	[bookmark: Text268]     
	square feet

	
	
	|_| My cleaning machine has no solvent/air interface.



	3.
	Tank description (Model No., Serial No., etc.):
	     



	4.
	Equipment standard compliance method chosen:
	|_| Control Combination (see pages 3-4)

	
	
	
	|_| Idling Emission Limit (see page 5*)
*Please ensure your idling emission limit test report(s) are attached.

	
	
	
	


General Instructions for Control Combination or Idling Emission Limit Equipment Standards
In filling out this packet, keep in mind that whether you choose the control combination or the idling emission limit equipment standard, the following should be included in each report for each machine, if it applies:
· A list of parameters that are to be monitored and the values of these parameters measured on or during the first month after the compliance date for each piece of control equipment on your machine that is required to be monitored.
· Compliance Date for Existing Machines:  December 2, 1997
· Compliance Date for New Machines:  At start-up or December 2, 1994, whichever is later.
· If you used reduced room draft as a control option, you need to report the conditions that must be maintained to comply with the windspeed requirement (i.e., enclosure, closed doors, closed windows).
· If you choose to comply with the idling emission limit, you need to submit an idling emission limit test report for tests of idling emissions (this test report can come from the vendor or manufacturer of your machine).
For each of the controls that are used to comply with the control combination or idling emission limit options, there are specific design, monitoring, and recordkeeping requirements. These are in the table titled Control Combination Device Requirements and should be attached with this packet. 
· The Design Requirements are necessary to define the controls and ensure that each control is capable of fulfilling its intended purpose.
· The Monitoring Requirements are necessary to make sure the equipment is working properly.
· The Recordkeeping is necessary to document the results of installation, monitoring, and determination results.
· If you use a control to comply with the idling emission limit that is not included in this packet, you must submit design, monitoring and recordkeeping requirements to the MPCA for approval. This information must be submitted with your idling emission standard test report.
	5.
	Control Combinations for Batch Vapor Cleaning Machines

	
	If you have a batch vapor cleaning machine:

	
	· and your solvent/air interface area is less than or equal to 1.21 square meters or 13 square feet; 
· and you have picked the control combination option for complying with this rule; 
· then, choose one of the following control option numbers for this machine:



	
	Control Combination Option number
	Working mode cover
	1.0 Freeboard ratio
	Super heated vapor
	Freeboard refrigeration
	Reduced room draft
	Carbon adsorber
	Dwell

	
	1
	X
	X
	X
	
	
	
	

	
	2
	
	
	X
	X
	
	
	

	
	3
	X
	
	
	X
	
	
	

	
	4
	
	X
	X
	
	X
	
	

	
	5
	
	
	
	
	
	
	

	
	6
	
	
	
	X
	X
	
	

	
	7
	
	
	
	X
	
	
	

	
	8
	
	X
	
	
	X
	
	X

	
	9
	
	
	
	X
	
	X
	

	
	10
	
	X
	X
	
	
	X
	



	
	What Option Number have you chosen for this machine?
	[bookmark: Text272]     
	



	
	If you have a batch vapor cleaning machine:

	
	· and your solvent/air interface area is less than or equal to 1.21 square meters or 13 square feet; 
· and you have picked the control combination option for complying with this rule; 
· then, choose one of the following control option numbers for this machine:



	
	Control Combination Option number
	Working mode cover
	1.0 Freeboard ratio
	Super heated vapor
	Freeboard refrigeration
	Reduced room draft
	Carbon adsorber
	Dwell

	
	1
	
	X
	X
	X
	
	
	

	
	2
	
	
	
	X
	X
	
	X

	
	3
	X
	
	X
	X
	
	
	

	
	4
	
	X
	X
	
	X
	
	

	
	5
	
	
	X
	X
	X
	
	

	
	6
	
	X
	
	X
	X
	
	

	
	7
	
	
	X
	X
	
	X
	



	
	What Option Number have you chosen for this machine?
	     
	



	
	If you have a batch vapor cleaning machine:

	
	· and your solvent/air interface area is less than or equal to 1.21 square meters or 13 square feet; 
· and you have picked the control combination option for complying with this rule; 
· then, choose one of the following control option numbers for this machine:



	
	Control Combination Option number
	Working mode cover
	1.0 Freeboard ratio
	Super heated vapor
	Freeboard refrigeration
	Reduced room draft
	Carbon adsorber
	Dwell

	
	1
	
	X
	X
	X
	
	
	

	
	2
	
	
	
	X
	X
	
	X

	
	3
	X
	
	X
	X
	
	
	

	
	4
	
	X
	X
	
	X
	
	

	
	5
	
	
	X
	X
	X
	
	

	
	6
	
	X
	
	X
	X
	
	

	
	7
	
	
	X
	X
	
	X
	



	
	What Option Number have you chosen for this machine?
	     
	



	6.
	Control Combinations for In-Line Cleaning Machines

	
	If you have an existing in-line cleaning machine:

	
	· and you have chosen the Control Combination option to comply with this rule;
· then choose one of the following control options for this machine:



	
	Control Combination Option number
	1.0 Freeboard ratio
	Super heated vapor
	Freeboard refrigeration
	Carbon adsorber
	Dwell

	
	1
	X
	X
	
	
	

	
	2
	X
	
	X
	
	

	
	3
	
	
	X
	
	X

	
	4
	
	
	
	X
	X



	
	What Option Number have you chosen for this machine?
	     
	



	
	If you have a new in-line cleaning machine:

	
	· and you have chosen the Control Combination option to comply with this rule; 
· then choose one of the following control options for this machine:



	
	Control Combination Option number
	1.0 Freeboard ratio
	Super heated vapor
	Freeboard refrigeration
	Carbon adsorber
	Dwell

	
	1
	
	X
	X
	
	

	
	2
	
	
	X
	X
	

	
	3
	
	X
	
	X
	



	
	What Option Number have you chosen for this machine?
	     
	



	7.
	Idling Emission Limits

	
	As an alternative to the previously listed control combinations, you can choose to comply with the idling emission limit option. To do this, you must meet an emission limit that is measured while the machine is idling (i.e., turned on, but not actively cleaning parts).

	
	· It is expected that the manufacturers will provide the idling emission rates for the machines they manufacture.
· If this service is not provided, then you must use TEST METHOD 307 to determine the idling emission rates for your machines. (Idling emissions are to be measured under idling conditions.)

	
	Idling Emission Rates for Batch Vapor Machines

	
	· 0.22 kg per hour per square meter or 0.045 pounds per hour per square foot of solvent/air interface area

	
	Idling Emission Rates for In-Line Cleaning Machines

	
	· 0.10 kg per hour per square meter or 0.021 pounds per hour per square foot of solvent/air interface area

	
	If you choose the idling emission limits to comply with the regulation and you choose parameters for controls not listed in the table titled Control Combination Device Requirements included with this packet, then you must submit design, monitoring and recordkeeping requirements to the MPCA for approval. This information must be submitted with your idling emission standard test report.



	8.
	For all facilities with Halogenated Solvent Cleaning Machines, please fill in the following information for this halogenated solvent cleaning machine:



	
	Halogenated Solvent
	Annual Consumption* for 1997 (in lbs)
	Annual Consumption for
1996 (in lbs)

	
	Methylene Chloride (CAS# 75-09-2)
	[bookmark: Text273]     
	     
	|_| Actual
	|_| Estimated

	
	Perchloroethylene (CAS# 127-18-4)
	     
	     
	|_| Actual
	|_| Estimated

	
	Trichloroethylene (CAS# 79-01-6)
	     
	     
	|_| Actual
	|_| Estimated

	
	1,1,1-Trichloroethane (Methyl Chloroform) (CAS# 71-55-6)
	     
	     
	|_| Actual
	|_| Estimated

	
	Carbon Tetrachloride (CAS# 56-23-5)
	     
	     
	|_| Actual
	|_| Estimated

	
	Chloroform (CAS# 67-66-3)
	     
	     
	|_| Actual
	|_| Estimated



	
	*Consumption means the amount of halogenated hazardous air pollutant solvent added to the solvent cleaning machine.

	
	· If you use actual annual consumptions for 1996, fill in the amount and check the “actual” box.  
· If you do not have actual annual consumption records for 1996, give us your best estimate for the amounts and check the “estimated” box.
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