	[image: New mm Logo for Forms]
	TF-09
Compliance Method Change Report – 
Control Combination or Idling Emission Limit
Halogenated Solvent Cleaning Equipment
Air Quality Permit Program
Doc Type: Notification


Instructions: Submit completed report to both:
	Minnesota Pollution Control Agency
AQ Compliance Tracking Coordinator:
AQRoutineReport.PCA@state.mn.us

	Chief, Air Enforcement & Compliance Assurance Branch
AE-17J
U.S. EPA Region 5
77 West Jackson Boulevard
Chicago, IL 60604-3507


For assistance, call:
	For businesses with 100 or fewer employees:
Small Business Assistance Program
Metro: 651-282-6143; Statewide: 800-657-3938
	For other facilities:
MPCA Customer Assistance Center
Metro: 651-296-6300; Statewide: 800-657-3864



	AI ID:
	     
	  Leave blank if you do not have this number.



	Facility name:
	     

	Street address:
	     
	County:
	     

	City:
	     
	State:
	     
	Zip code:
	     


Facility Contact Person
	Name:
	     
	Title:
	     

	Email:
	     
	Phone:
	     
	Fax:
	     


Responsible Official
	Name:
	     
	Title:
	     

	Signature:
	
	Date (mm/dd/yyyy):
	     



	Effective date (mm/dd/yyyy):
	     
	, I have officially changed my Equipment Standard Compliance Method.

	From:
	|_| Control Combination
	|_| Idling Emission Limit

	To:
	|_| Control Combination (see pages 2 and 3)
	|_| Idling Emission Limit (see page 3; ensure your compliance report is attached)





Cleaning machine description(s) Fill out a separate form for each solvent cleaning machine.
	1. 
	Facility’s machine identification no.:
	     

	
	Manufacturer:
	[bookmark: Text296]     

	
	Model no.:
	     
	

	
	Serial no.
	[bookmark: Text295]     
	

	
	Date of installation:
	[bookmark: Text297]     
	

	
	Type of cleaning machine:
	|_| Existing (Construction or reconstruction began on or before November 29, 1993)

	
	
	|_| New (Construction or reconstruction began after November 29, 1993)

	
	
	|_| Batch Vapor   |_| In-Line

	
	Solvent/air interface area is:
	     
	 square feet
	or
	     
	 square meters

	
	|_| My cleaning machine has no solvent/air interface.



	2. 
	Facility’s machine identification no.:
	     

	
	Manufacturer:
	     
	

	
	Model no.:
	     
	

	
	Serial no.
	     
	

	
	Date of installation:
	     
	

	
	Type of cleaning machine:
	|_| Existing (Construction or reconstruction began on or before November 29, 1993)

	
	
	|_| New (Construction or reconstruction began after November 29, 1993)

	
	
	|_| Batch Vapor   |_| In-Line

	
	Solvent/air interface area is:
	     
	 square feet
	or
	     
	 square meters

	
	|_| My cleaning machine has no solvent/air interface.



	3. 
	Facility’s machine identification no.:
	     

	
	Manufacturer:
	     
	

	
	Model no.:
	     
	

	
	Serial no.
	     
	

	
	Date of installation:
	     
	

	
	Type of cleaning machine:
	|_| Existing (Construction or reconstruction began on or before November 29, 1993)

	
	
	|_| New (Construction or reconstruction began after November 29, 1993)

	
	
	|_| Batch Vapor   |_| In-Line

	
	Solvent/air interface area is:
	     
	 square feet
	or
	     
	 square meters

	
	|_| My cleaning machine has no solvent/air interface.



	4. 
	Facility’s machine identification no.:
	     

	
	Manufacturer:
	     
	

	
	Model no.:
	     
	

	
	Serial no.
	     
	

	
	Date of installation:
	     
	

	
	Type of cleaning machine:
	|_| Existing (Construction or reconstruction began on or before November 29, 1993)

	
	
	|_| New (Construction or reconstruction began after November 29, 1993)

	
	
	|_| Batch Vapor   |_| In-Line

	
	Solvent/air interface area is:
	     
	 square feet
	or
	     
	 square meters

	
	|_| My cleaning machine has no solvent/air interface.






	
	Control Combinations for Batch Vapor Cleaning Machines

	
	If you have a batch vapor cleaning machine:

	
	· and your solvent/air interface area is less than or equal to 1.21 square meters or 13 square feet; 
· and you have picked the control combination option for complying with this rule; 
· then, choose one of the following control option numbers for this machine:



	
	Control Combination Option number
	Working mode cover
	1.0 Freeboard ratio
	Super heated vapor
	Freeboard refrigeration
	Reduced room draft
	Carbon adsorber
	Dwell

	
	1
	X
	X
	X
	
	
	
	

	
	2
	
	
	X
	X
	
	
	

	
	3
	X
	
	
	X
	
	
	

	
	4
	
	X
	X
	
	X
	
	

	
	5
	
	
	
	X
	X
	
	

	
	6
	
	
	
	X
	
	
	

	
	7
	
	
	
	X
	
	
	X

	
	8
	
	X
	
	
	X
	
	X

	
	9
	
	
	
	X
	
	X
	

	
	10
	
	X
	X
	
	
	X
	



	
	What Option Number have you chosen for this machine?
	[bookmark: Text272]     
	



	
	If you have a batch vapor cleaning machine:

	
	· and your solvent/air interface area is less than or equal to 1.21 square meters or 13 square feet; 
· and you have picked the control combination option for complying with this rule; 
· then, choose one of the following control option numbers for this machine:



	
	Control Combination Option number
	Working mode cover
	1.0 Freeboard ratio
	Super heated vapor
	Freeboard refrigeration
	Reduced room draft
	Carbon adsorber
	Dwell

	
	1
	
	X
	X
	X
	
	
	

	
	2
	
	
	
	X
	X
	
	X

	
	3
	X
	
	X
	X
	
	
	

	
	4
	
	X
	X
	
	X
	
	

	
	5
	
	
	X
	X
	X
	
	

	
	6
	
	X
	
	X
	X
	
	

	
	7
	
	
	X
	X
	
	X
	



	
	What Option Number have you chosen for this machine?
	     
	



	
	Control Combinations for In-Line Cleaning Machines

	
	If you have an existing in-line cleaning machine:

	
	· and you have chosen the Control Combination option to comply with this rule;
· then choose one of the following control options for this machine:



	
	Control Combination Option number
	1.0 Freeboard ratio
	Super heated vapor
	Freeboard refrigeration
	Carbon adsorber
	Dwell

	
	1
	X
	X
	
	
	

	
	2
	X
	
	X
	
	

	
	3
	
	
	X
	
	X

	
	4
	
	
	
	X
	X



	
	What Option Number have you chosen for this machine?
	     
	



	
	If you have a new in-line cleaning machine:

	
	· and you have chosen the Control Combination option to comply with this rule; 
· then choose one of the following control options for this machine:



	
	Control Combination Option number
	1.0 Freeboard ratio
	Super heated vapor
	Freeboard refrigeration
	Carbon adsorber
	Dwell

	
	1
	
	X
	X
	
	

	
	2
	
	
	X
	X
	

	
	3
	
	X
	
	X
	



	
	What Option Number have you chosen for this machine?
	     
	



	
	Idling Emission Limits

	
	If you have chosen to comply with the idling emission limit option, you must meet an emission limit that is measured while the machine is idling (i.e., turned on, but not actively cleaning parts).  The manufacturer or vendor can usually provide the idling emission rate for the machine.

	
	Otherwise:

	
	· You must use Test Method 307 to determine the idling emission rate for your machine (idling emissions are to be measured under idling conditions).

	
	Idling Emission Rates for Batch Vapor Machines

	
	· 0.22 kg per hour per square meter or 0.045 pounds per hour per square foot of solvent/air interface area

	
	Idling Emission Rates for In-Line Cleaning Machines

	
	· 0.10 kg per hour per square meter or 0.021 pounds per hour per square foot of solvent/air interface area

	
	If you have chosen the idling emission limits to comply and you have chosen parameters for controls not listed in paragraphs (a) through (e) of Section 63.466 Monitoring Procedures, then you must submit design, monitoring and recordkeeping requirements to the MPCA for approval. This information must be submitted with your idling emission test report.
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