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	TF-01
Initial Statement of Compliance Report - 
Alternative Standard/Overall Emission Limit
Halogenated Solvent Cleaning Equipment
Air Quality Permit Program
Doc Type: Notification


Instructions: This report must be postmarked or received by the applicable due date, located at the bottom of this page. Submit completed report to both:
	Minnesota Pollution Control Agency
AQ Compliance Tracking Coordinator:
AQRoutineReport.PCA@state.mn.us

	George Czerniak
AE-17J
U.S. EPA Region 5
77 West Jackson Boulevard
Chicago, IL 60604-3507



	AI ID:
	[bookmark: Text118]     
	Date (mm/dd/yyyy):
	[bookmark: Text262]     

	Facility name:
	     


Facility address
	Street address:
	     
	County:
	     

	City:
	     
	State:
	     
	Zip code:
	     


Mailing address
	Street address:
	     
	
	

	City:
	     
	State:
	     
	Zip code:
	     



	Facility contact person:
	     
	Phone number:
	[bookmark: Text272]     

	Title:
	[bookmark: Text263]     
	


Responsible official
	Name:
	[bookmark: Text119]     
	
	

	Title:
	     
	
	

	Signature:
	
	Date (mm/dd/yyyy):
	[bookmark: Text264]     


Cleaning machine (fill out separate form for each solvent tank)
	1.
	Tank Identification No.:
	[bookmark: Text265]     
	

	
	Date of tank installation (mm/dd/yyyy):
	[bookmark: Text266]     
	

	
	Tank is:
	|_| Existing
	(This report is due by May 1, 1998)

	
	
	|_| New
	(This report is due 150 days after start-up or May 1, 1995, whichever is later)



	2.
	Type of machine:
	|_| Batch vapor
	

	
	
	|_| In-Line
	



	
	Solvent/Air Interface area:
	[bookmark: Text267]     
	square meters

	
	
	or
	

	
	
	[bookmark: Text268]     
	square feet

	
	
	|_| My cleaning machine has no solvent/air interface.



	3.
	Tank description (Model No., Serial No., etc.):
	     



	4.
	Cleaning capacity of your machine:
	     
	cubic meters

	
	
	or
	

	
	
	     
	cubic feet


General Instructions for Overall Emission Limit Also Known As Alternative Standard
· This option allows you the flexibility to establish your own emission-reduction strategy provided you comply with the overall emission limit.
· Applicable overall emission limits are based on your cleaning machine type and size.
· If you comply with the limit specified for your machine, you do not have to follow any additional equipment monitoring or work practice requirements.
· In addition, operators of machines complying with this option are not subject to the solvent cleaning procedures test. This is a test that the MPCA can give during an inspection. This test ensures that each operator has adequate knowledge of solvent cleaning operating procedures. Each operator of a solvent cleaning machine must complete and pass applicable sections of a solvent cleaning procedures test, when requested by the MPCA.
· This option is generally easiest to comply with when a machine is either well-controlled or infrequently used.
To determine the 3-month average monthly emission limit for your machine, multiply the solvent/air interface area (size) of the machine by the applicable limit (shown in table below):
	Machine Type
	3-Month Average Monthly
Emission Limit (kg/m2 x month)a
	3-Month Average Monthly
Emission Limit (lbs/ft2 x month)b

	Batch Vapor
	150
	30.7

	Existing In-Line
	153
	31.4

	New In-Line
	99
	20


a	m2 = The total surface area of all cleaning tanks for a particular machine (i.e., solvent/air interface area).
b	ft2 = The total surface area of all cleaning tanks for a particular machine (i.e., solvent/air interface area).

If your machine does not have a solvent/air interface area:
· Your emission limit is based on your machine’s cleaning capacity. 
· An emissions limit based on your machine’s cleaning capacity is only an option if your machine does not have a solvent/air interface area.
· An emission limit based on your machine’s cleaning capacity is not a compliance option for a machine with a solvent/air interface area.
Determine your machine’s cleaning capacity in one of the following ways:
	Check the literature that was provided with your machine at the time of purchase to see if it includes a measurement of the cleaning capacity for your cleaning machine;

	or

	Ask the manufacturer of your machine for the cleaning capacity;

	or

	Determine the cleaning capacity of your machine from the following information:

	· The internal width (IW) (specify meters or feet) of the cleaner tank;
· The internal width (IW) (specify meters or feet) of the cleaner tank;
· The internal length (IL) (specify meters or feet) of the cleaner tank; and
· The depth (D) (specify meters or feet) of the cleaner tank.
· The cleaning capacity is obtained by multiplying the above numbers together (i.e., Capacity = IW x IL x D)



Records of the cleaning capacity determination for each of your machines without a solvent/air interface are to be maintained on‑site in paper or electronic form for the lifetime of the machine.
	5.
	If your machine does not have a solvent/air interface area, explain the calculation methods and the results used to determine the cleaning capacity of your machine: (attach a separate sheet of paper, if necessary)

	
	[bookmark: Text269]     

	
	     

	
	     

	
	     

	
	     



	6.
	The first 3 month average emissions for this machine is:
	     
	kg/month

	
	
	or
	

	
	(Calculation sheets should be attached.)
	     
	lb/month



	7.
	For all facilities with halogenated solvent cleaning machines, please fill in the following information:



	
	Halogenated Solvent
	Annual Consumption* for 1997 (in lbs)
	Annual Consumption
for 1996 (in lbs)

	
	Methylene Chloride (CAS# 75-09-2)
	     
	[bookmark: Text270]     
	|_| Actual
	|_| Estimated

	
	Perchloroethylene (CAS# 127-18-4)
	     
	[bookmark: Text271]     
	|_| Actual
	|_| Estimated

	
	Trichloroethylene (CAS# 79-01-6)
	     
	     
	|_| Actual
	|_| Estimated

	
	1,1,1-Trichloroethane (Methyl Chloroform) (CAS# 71-55-6)
	     
	     
	|_| Actual
	|_| Estimated

	
	Carbon Tetrachloride (CAS# 56-23-5)
	     
	     
	|_| Actual
	|_| Estimated

	
	Chloroform (CAS# 67-66-3)
	     
	     
	|_| Actual
	|_| Estimated

	
	*Consumption means the amount of halogenated hazardous air pollutant solvent added to the solvent cleaning machine.

	
	· If you use actual annual consumptions for 1996, fill in the amount and check the “actual” box.  
· If you do not have actual annual consumption records for 1996, give us your best estimate for the amounts and check the “estimated” box.
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